#
# J-LINK GDB SERVER initialization
#
target remote localhost:2331
set remotetimeout 10000
monitor device Cortex-M3
monitor endian little
monitor reset
# Set max speed
monitor speed 4000
set mem inaccessible-by-default off
# Setup GDB FOR FASTER DOWNLOADS
#set remote memory-write-packet-size 4096
#set remote memory-write-packet-size fixed
# Boot Flash
monitor long 0x40000210 = 0x211157
# Boot RAM start_addr0() Run if ( v400001F4 & 0x8000000 ) && ( v40000210 & 0x80000000 ) 
#monitor long 0x40000210 = 0x80011117
# Boot RAM start_addr1() Run if ( v40000210 & 0x20000000 ) 
#monitor long 0x40000210 = 0x20011117
# Boot RAM start_addr2() Run if ( v40000210 & 0x10000000 )
#monitor long 0x40000210 = 0x10011117
# Boot RAM start_addr3() Run if ( v400001F4 & 0x8000000 ) && ( v40000210 & 0x8000000 )
#monitor long 0x40000210 = 0x8011117
# Boot RAM start_addr4() Init console, Run if ( v40000210 & 0x4000000 )
monitor long 0x40000210 = 0x4011117
# CPU CLK 166 MHz?
# monitor long 0x40000014 = 0x00000011 
# CPU CLK 83 MHz?
#monitor long 0x40000014 = 0x00000021 
