(module TerminalBlock:TerminalBlock_bornier-4_P5.08mm (layer F.Cu) (tedit 59FF03D1)
  (descr "simple 4-pin terminal block, pitch 5.08mm, revamped version of bornier4")
  (tags "terminal block bornier4")
  (fp_text reference J2 (at 7.6 -4.8) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Conn_01x04_Male (at 7.6 4.75) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text user %R (at 7.62 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.48 2.55) (end 17.72 2.55) (layer F.Fab) (width 0.1))
  (fp_line (start -2.43 3.75) (end -2.48 3.75) (layer F.Fab) (width 0.1))
  (fp_line (start -2.48 3.75) (end -2.48 -3.75) (layer F.Fab) (width 0.1))
  (fp_line (start -2.48 -3.75) (end 17.72 -3.75) (layer F.Fab) (width 0.1))
  (fp_line (start 17.72 -3.75) (end 17.72 3.75) (layer F.Fab) (width 0.1))
  (fp_line (start 17.72 3.75) (end -2.43 3.75) (layer F.Fab) (width 0.1))
  (fp_line (start -2.54 -3.81) (end -2.54 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 17.78 3.81) (end 17.78 -3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start 17.78 2.54) (end -2.54 2.54) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.54 -3.81) (end 17.78 -3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.54 3.81) (end 17.78 3.81) (layer F.SilkS) (width 0.12))
  (fp_line (start -2.73 -4) (end 17.97 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.73 -4) (end -2.73 4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 17.97 4) (end 17.97 -4) (layer F.CrtYd) (width 0.05))
  (fp_line (start 17.97 4) (end -2.73 4) (layer F.CrtYd) (width 0.05))
  (pad 2 thru_hole circle (at 5.08 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 10.16 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
  (pad 1 thru_hole rect (at 0 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
  (pad 4 thru_hole circle (at 15.24 0) (size 3 3) (drill 1.52) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/TerminalBlock.3dshapes/TerminalBlock_bornier-4_P5.08mm.wrl
    (offset (xyz 7.619999885559082 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
