ADELSYSTEM_CBI(8)
=================

NAME
----

adelsystem_cbi - Driver for the ADELSYSTEM CB/CBI DC-UPS

SYNOPSIS
--------

*adelsystem_cbi* -h

*adelsystem_cbi* -a 'DEVICE_NAME' ['OPTIONS']

NOTE: This man page only documents the specific features of the *adelsystem_cbi*
driver. For information about the core driver, see linkman:nutupsdrv[8].

SUPPORTED HARDWARE
------------------

This is the driver for the adelsystem cb/cbi dc-ups devices.

The driver has been tested against CBI2801224A, all in one 12/24Vdc DC-UPS.

More information about this UPS can be found here: ::
https://www.adelsystem.com/en/products/dc-ups-/


EXTRA ARGUMENTS
---------------

This driver supports the following optional settings in the
linkman:ups.conf[5] file:

Serial:
~~~~~~

*ser_baud_rate*='value'::
A integer specifying the serial port baud rate (default 9600).

*ser_data_bit*='value'::
A integer specifying the serial port data bit (default 8).

*ser_parity*='value'::
A character specifying the serial port parity (default N).

*ser_stop_bit*='value'::
An integer specifying the serial port stop bit (default 1).

Modbus:
~~~~~~

*dev_slave_id*='value'::
An integer specifying the device modbus slave ID (default 1).


CONFIGURATION
-------------

Here is an example of adelsystem_cbi driver configuration in *ups.conf* file:
----
[adelsystem_cbi]
  driver = adelsystem_cbi
  port = /dev/ttyUSB0
  desc = "adelsystem cb/cbi ups driver"
  # serial settings
  ser_baud_rate = 9600
  ser_parity = N
  ser_data_bit = 8
  ser_stop_bit = 1
  # modbus slave id
  dev_slave_id = 5
----

INSTANT COMMANDS
----------------

This driver support the following instant commands:

load.off::
executes "instant poweroff"

INSTALLATION
------------

This driver is not built by default. You can build it by installing
libmodbus and running `configure --with-modbus=yes`.

You also need to give proper permissions on the local serial device
file (/dev/ttyUSB0 for example) to allow the run-time NUT driver user
account to access it.

AUTHOR
------

Dimitris Economou <dimitris.s.economou@gmail.com>

SEE ALSO
--------

The core driver:
~~~~~~~~~~~~~~~~

linkman:nutupsdrv[8], linkman:ups.conf[5]

Internet resources:
~~~~~~~~~~~~~~~~~~~

* The NUT (Network UPS Tools) home page: http://www.networkupstools.org/
* libmodbus home page: http://libmodbus.org
